MODEL 200HRS-150 DIGITAL DISPLAY ROCKWELL HARDNESS TESTER
 
Feature & Use:
· [bookmark: OLE_LINK2]High quality integral casting cast iron machine body with automotive paint treatment process, the appearance is smooth and beautiful.
· The measuring device adopts grating displacement sensor, the test results are displayed on large LCD screen, the test scale, test force, indenter type, holding time and the conversion unit can be displayed and set.
· Convenient control system can automatically convert the unit of full hardness scale.
· The built-in test software can correct the measurement results of the machine by ±3HR.
· The loading, holding and unloading of the test force are controlled by motor, the manual operation error is eliminated.
· Equipped with blue-tooth printer, the data can be output through USB or RS232 port
· Precision conforms to GB/T230.2, ISO6508-2 and ASTM E18.
 
        It’s a kind of digital display type Rockwell hardness tester. It’s suitable to determine the Rockwell hardness of ferrous, non-ferrous metals and non-metal materials. It features wide application range, easy operation, good economy and practicality. It can be widely applied in the Rockwell hardness testing for heat treatment materials, such as quenching, hardening and tempering, etc.
 
Specifications:
 
Measuring range: 20-95HRA, 10-100HRBW, 20-70HRC
Test force: 588.4, 980.7, 1471N (60, 100, 150kgf)
Max. height of test piece: 200mm
Depth of throat: 160mm
Min. scale value: 0.1HR
Dwelling time: 1~99s
Power supply: 220V AC or 110V AC, 50 or 60Hz
Dimensions: 510 x 290 x 730mm
Weight: approx. 80kg
 
Standard accessories:
 
   Large flat anvil: 1 pc.
   Small flat anvil: 1 pc.
   V-notch anvil: 1 pc.
   Diamond cone penetrator: 1 pc
   1/16” Tungsten carbide ball penetrator: 1 pc.
   Rockwell standardized block: 5 pcs.
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